{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["大型精密分析仪器实验室设备配置"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"大型精密分析仪器实验室设备配置","index":0,"n_rows":17,"n_cols":13,"rows_kept":17,"merged":[[0,0,0,11]],"flags":["formulas_cached_only"]}
["大型精密分析仪器实验室设备配置（2018年4月）"]
["序号","实验室名称","资产条码","资产名称","型号规格","技术指标","单价","生产厂家","生产国别","使用方向","经费来源","保管人","存放地点"]
[1,"XRD分析实验室","（尚未未打印）","多功能X射线衍射仪","荷兰帕纳科X'Pert3 Powder ",null,1039170,null,"荷兰","科研","中央财政专项资金","张恒","化工楼-022"]
[2,"扫描电镜分析实验室","2015014754","台式扫描电镜","VEGA3-SBH","放大倍率：4.5倍－1000,000倍，可连续调整",994000,"捷克TESCAN","捷克","科研","中央财政专项资金","陈卓","化工楼-023"]
[3,"色谱分析实验室","2014003410","气相色谱-质谱联用仪","7890A/5975C","质量数范围：1.6～1050amu，以0.1amu递增",657000,"美国安捷伦科技有限公司","美国","教学","中央财政专项资金","司甜","化工楼-028"]
[4,"元素分析实验室","2017002040","等离子体发射光谱仪","optima8000","在200nm处时，光学分辨率为≤0.007nm",550000,"美国珀金埃尔默仪器有限公司","美国","科研","中央财政专项资金","张恒","化工楼-024"]
[5,"热分析实验室","80027586","同步热分析仪","STA449F3","最大称重量：10g",540000,"耐驰仪器制造公司","德国","教学","教学设备费","陶军","化工楼-025"]
[6,"元素分析实验室","2017002041","全自动元素分析仪","EA2400II","测试精确度0.2%分析用Ar时准确度≤0.5%精度≤0.4%",495000,"美国珀金埃尔默仪器有限公司","美国","科研","中央财政专项资金","张恒","化工楼-024"]
[7,"色谱分析实验室","20164d0251","原位傅里叶红外光谱仪","VERTEX 70","分辨率：0.2 cm-1，连续可调,信噪比：优于50,000:1;光谱范围：8,000-50 cm-1 ",373934.61,"布鲁克香港有限公司","德国","教学","德元贷款","司甜","化工楼-028"]
[8,"色谱分析实验室","2015002893","气相色谱",null,null,300000,"岛津","日本","教学","中央财政专项资金","陶军","化工楼-028"]
[9,"光谱分析实验室","20090684","液相色谱","安捷伦1200","流速＜0.07％RSD",299880,"安捷伦公司","美国","教学","教学设备费","司甜","化工楼-026"]
[10,"光谱分析实验室","20164d0191","纳米粒度、电位和分子量测定仪","Zetasizer NANO ZS90","粒子测定方法：采用经典的DLS方法,测量范围：0.3nm~6μm；ZETA电位可测量粒径范围：3 nm~100 μm；",266808.66,"马尔文仪器公司","英国","教学","德元贷款","司甜","化工楼-026"]
[11,"热分析实验室","2014003409","量热仪","C2000","测量范围：最大可达40,000J；温度分辨率：0.0001℃",265000,"德国IKA公司","德国","教学","中央财政专项资金","陶军","呈贡校区-化工楼-025"]
[12,"电化学分析实验室","2014003411","全自动旋光仪","Autopol I-S2","测量范围：±89.99°Arc；浓度：0～99.9%",199000,"美国鲁道夫公司","美国","教学","中央财政专项资金","赵榆林","化工楼-027"]
[13,"电化学分析实验室","2012002278","表面张力仪","SL200B","接触角测量范围0-180°，接触角分辨率0.01°",156000,"美国科诺工业有限公司","中国","教学","科研基础平台经费","赵榆林","化工楼-027"]
[14,"热分析实验室","20164d0261","氧弹量热量仪","C200","用于测量液体和固体样品的热值，符合标准: DIN 51900,ISO 1928, ASTM D240, ASTM D4809, ASTM D5865, ASTM D1989",127636.82,"广州仪科实验室技术有限公司","中国","教学","德元贷款","陶军","化工楼-025"]
[{"$nulls":5},"合计",6263430.090000001]